PROJECT: _________________ REVIEWER: _____________ DATE: ________

STORM SEWER STRUCTURE

SHOP DRAWING CHECKLIST

__________	1.	APPROVED CONCRETE MIX DESIGN.

__________	2.	TYPE AND SIZE OF STEEL FRAME W/ DETAIL

(FRAME MUST BE GALVANIZED).

__________	3.	TYPE OF STEP AND DETAIL.

__________	4.	TYPE OF COVER W/ OVERLAND PARK LOGO.

__________	5.	REINFORCING DETAIL W/ EXTENSIONS ABOVE THE	WALL FOR POURED IN PLACE TOPS, WALL THICK-

NESS AND BASE DIMENSIONS.

__________	6.	TOP ELEVATION W/ LONGITUDINAL & CROSS SLOPE,

IF NECESSARY.

__________	7.	PIPE FLOWLINE ELEVATIONS ( IN AND OUT).

__________	8.	PIPE ALIGNMENT (TO CENTER OF

STRUCTURE)

__________	9.	JUNCTION BOX ELEVATIONS TO ALLOW FOR

LID COVER ADJUSTMENT RINGS.

__________	10.	DETERMINE IF THE ENTIRE STRUCTURE SHOULD BE	POURED IN PLACE TO PROTECT STRUCTURAL

INTEGRITY DUE TO SIZE AND NO. OF BLOCKOUTS.

__________	11.	MINIMUM OF 4” CONCRETE INVERT BELOW

OUTSIDE PIPE WALL & MINIMUM OF 2” CLEARANCE BETWEEN THE OUTSIDE PIPE WALL AND THE EDGE OF THE BLOCKOUT.

__________	12.	EACH STRUCTURE HAS A NUMBER & STRUCTURE

NUMBERS MATCH THOSE ON THE PLANS.

__________	13.	DETERMINE IF THE STRUCTURE SIZE WILL

ACCOMMODATE THE SIZE OF THE PIPE SHOWN.

__________	14.	LOCATION OF WEEP HOLES ( A MINIMUM OF 26”	FROM TOP OF THE STRUCTURE TO CTR. OF WEEP-

HOLES.)

storm sewer structure checklist

Kathie Petrie

1999-11-29

Joe Archer

City of Overland Park