August 12, 2008

Mark Holmes

Pyramid Contractors

765 W. Ironwood

Olathe, Ks. 66061

Metcalf Avenue (HWY US 169) Widening & Resurfacing

I-435 to 99th Street

KDOT# 169-46 N-0314-01

We have viewed the above-referenced project construction site and have the following items to be resolved prior to acceptance of this project:

Remove Silt fence and Straw Waddles along Metcalf lane.

Remove Control point #11

Remove and replace cracked sidewalk panel along Metcalf Lane west side of Metcalf.

Remove and Replace 2 Cracked panels of sidewalk on the SE corner of Metcalf.

Remove sand bag on the SW corner of 99th and Metcalf.

Remove and Replace cracked panel of sidewalk on the NW corner of Metcalf.

Remove sing post on the NW corner of 99th and Metcalf.

Remove only pavement markings in the old right turn lane which is now a through lane and restripe.

Backfill the sidewalk ramp wings on the NW corner of Metcalf.

Finish backfilling curb in the median on the north leg of Metcalf. Grade to drain to the north to area grate inlet.

Install inlet protection in the north median at 99th and Metcalf.

Clean up the trash in the medians.

Fill along the bike path where it has washed out and reseed.

Wedge the asphalt to match the concrete ramp on the NE corner of 99th and Metcalf.

Backfill the east ramp on the NE corner of 99th and Metcalf.

Clean the silt of area inlet #208, and install a new straw waddle.

Place top soil around the ramp on the north end of the bike path near sears.

There are several valves and Manholes in the bike path adjust them and torch new asphalt in to smooth path. Between 99th and the Mall parking lot.

SE corner 99th and Metcalf place dirt around the manhole of junction box 801 and grade to drain.

Grade around the pole base on the south leg of the median at 99th and Metcalf.

Raise the Manhole and valve and place top soil around finish graded on the east side of the bike path around Sta. 162+00.

Remove the silt and straw waddles in Area inlets 702, 701, 204, and 401.

Contact Todd Gunther at K&W (913) 782-7387 to fix the sod on the east side of the bike path near 101st Street.

Cut the wire out of the North median at 101st Street.

Finish grade on the NW corner of 101st and Metcalf. Remove large dirt clods along the fence of the wing walls of the con span and hand grade.

Remove the straw waddle along the top of the wall in front of the church.

Finish the sidewalk ramp on the SW corner of 100st Street by Friday the 15th.

Finish grade between the con span and the RCB and again remove the large dirt clods along the rip and con span wing walls. (The Cities Definition of finish grading is 1 operator with a skid steer or machine of choice and 1 or 2 labors with shovels and rakes working together not separately to get the grade right removing trash and large rocks, ect. as they move along.) Once this is done reseed the disturbed area and mulch using a tackifier on top.

Clean Hydro-mulch from hand rail and wall along con span and RCB.

Grout the pipes in the RCB flush with the inside walls it the pipe does not reach the inside walls either use sona tube with steel reinforcement of install another section of pipe.

If you have any questions please contact the undersigned, or Brian Hammond.

Chris Hutton

Construction Inspector, Senior

cc:	Dan Miller, P.E., City Engineer

Larry Blankenship, P.E., Assistant City Engineer

punch list

Mary Lou McCann

2008-08-12

cahutton

City of Overland Park