**Testing Recap Log**

**Metcalf Avenue 151st to 135th Street**

**KDOT Project No.: 46 N 0186-01 OP Project No.: Th-0356**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Types of tests performed** | **Testing frequency** | **Quantity Totals** | **# of tests performed** | **Actual testing Frequency** | **Pass/Fail** | **Remarks** |
| Fly Ash | 1 per 600m2 | 90858m2 | 61 | 1 per 1489m2 | 52/9 | See note 1. Retests passed |
| **CONCRETE** |  |  |  |  |  |  |
| Structures | 1 per 50m3 | 141m3 | 12 | 1 per 12m3 | 12/0 |  |
| Curb | 1 per 150m | 13721.16m | 22 | 1 per 623m | 21/1 | See note 1. Retest passed |
| Sidewalk | 1 per 500m2 | 7096.07 | 9 | 1 per 788m2 | 9/0 | See note 1. |
| Drives | 1 per 500m2 | 1879.00m2 | 3 | 1 per 626m2 | 3/0 | See notes 1 & 2. |
| **GRADATION** |  |  |  |  |  |  |
| OP Special | 1 per 1000t | 18459.83 | 16 | 1 per 1153t | 14/2 | Retest passed |
| Edge Drain | 1 per 250t |  | 2 |  | 2/0 | See note 3. |
| Storm Sewer and BD-1 |  |  | 4 |  | 3/1 | See note 4.Retest passed |
| Asphalt | As per Engineer | 48266.57t | 41 | 1 per 1177t | 41/0 | See note 5. |
| Compaction of Soils | 1 per 600m2 | 56752m3 | 61 | 1 per 930m3 | 49/12 | See note 6. |

Notes:

1. Tested at beginning of daily run and as needed there after.
2. Most drives poured at same time as curb.
3. Tested per phase, most delivered at one time for each phase.
4. No specified testing frequency. Tested for assurance.
5. Tested once in AM and PM or as needed.
6. Tested per lift or at least twice daily.

Refer to log notes or testing reports for reasons of test failures.

Kevin J. Shaunty

Construction Inspector, Senior