November 15, 1999

Max Brashears

Reno Construction Company

A Division of APAC-Kansas, Inc.

Post Office Box 23910

Overland Park, KS 66223

ANTIOCH ROAD – 143RD STREET TO 151ST STREET (City of OP Project Number)

CORRECTIONS REQUIRED AT END OF THE ONE YEAR MAINTENANCE PERIOD

Inspection was made on the above referenced project on October 21, 1999. Following is a punch list of items that need to be corrected:

Repair cracked curb inlet transitions at the following locations:

Station 59+93, 41.5’ Left (1 transition)

Station 75+30, 41.5’ Left (2 transitions)

Station 78+44.79, 41.5’ Right (1 transition)

Station 78+45.64, 41.5’ Left (2 transitions)

Station 82+50, 41.5’ Left (2 transitions)

Station 82+50, 41.5’ Right (1 transition)

Station 92+00, 41.5’ Right (2 transitions)

Station 93+75, 41.5’ Left (2 transitions)

Station 95+50, 41.5’ Right (2 transitions)

Station 10+78.50, 15.5’ Right, 144th Street (2 transitions)

Station 10+80.50, 15.5’ Left, 144th Street (2 transitions)

Replace cracked curb at the following locations:

Southwest radius at 148th Street

Northwest radius at 148th Street

West side of Antioch Road at 147th Terrace

Northeast radius at 147th Terrace

Southeast radius at 147th Terrace

East side of Antioch Road 100’ North of 147th Terrace

West side of Antioch Road 150’ North of 147th Street (2 locations)

West side of Antioch Road 100’ North of school speed limit sign North of 147th Street (2 locations)

East side of Antioch Road 50’ North of first curb inlet North of 147th Street

Southeast corner of 144th Street

In front of 14330 Antioch Road

In front of 14316 Antioch Road

Max Brashears

Page Two

November 15, 1999

Replace cracked sidewalk at the following locations:

Southeast corner at 147th Street

Near North end of form liner wall (patched before)

Remove silt fence by the storm sewer outlet structure at Station 86+00.

Repair cracked integral sidewalk retaining wall at expansion joint near 148th Street intersection.

Reset paving brick drive along curb on 148th Street.

7.	Repair anchor holes in sidewalk at face of integral sidewalk retaining wall.

Brian Hammond will be available to answer your questions regarding the items noted above.

WAYNE A. GUDENKAUF, P.E.

CIVIL ENGINEER II

js

cc:	Brian Hammond – Construction Operations Specialist

Email:	William D. Brown, P.E. – City Engineer

Daniel G. Miller, P.E. – Supervisory Civil Engineer

maintenance inspection

Wayne Gudenkauf

2000-01-13

Joe Archer

City of Overland Park